1. **Test Dataset: AA400015**

**S‐58 Recommended ENC Validation Checks covered in this section:**

|  |  |
| --- | --- |
| **S‐58 Check** | **Description** |
| 24 | For each SOUNDG feature object which does not reference a SG3D field with X, Y and Z values. |
| 26a | For each subfield where the value is not within the range defined in the S-57 format description. |
| 536 | If a field without a repetition factor repeats. |
| 540a | If mandatory records, fields and subfields are not Present OR are Null where the “Null” value is not allowed. |
| 540b | If data set file contains prohibited records, fields or subfields. |

**Secondary Errors**

Critical – 27, 555,

Error –

Warnings –

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Dataset Name** | AA400015 | | | **S‐58 Check** | | 24 | | | **Type** | | C |
| **S-58 Description** | For each SOUNDG feature object which does not reference a SG3D field with X, Y and Z values. | | | | | | | | | | |
| **Message** | SOUNDG does not reference a SG3D field. | | | | | | | | | | |
| **Solution** | Amend coordinate type or values for SOUNDG. | | | | | **Conformity** | | Part 3 (5.1.4.1) | | | |
| **Test Case No. 1** | Revised SG3D to SG2D for SOUNDG feature. | | | | | | | | | | |
| **Location** | | **Feature** | **Attributes** | | **FRID** | | **FOID** | | | **VRID** | |
| - | | SOUNDG |  | | FE-48 | |  | | |  | |
| **Location** | 32°33'34.53"S 61°11'40.74"E | | | **S57 Encoding** | | SOUNDG | |  | | | |
| **FOID or VRID** | FE-000048 | | |  | |  | |  | | | |
| **Screen Capture** |  | | | | | | | | | | |
| **Expected Test Results** | 24: An error “SOUNDG does not reference a SG3D field.” must be triggered. | | | | | | | | | | |
| **Secondary Critical Errors** | 20: An error “Geometric primitive of this type is not permitted for this object class” must be triggered.  21: An error “orphan which is the edge is dose not point to end node” must be triggered. | | | | | | | | | | |
|  | | | | | | | | | | | |
| **Dataset Name** | AA400015 | | | **S‐58 Check** | | 26a | | | **Type** | | C |
| **S-58 Description** | For each subfield where the value is not within the range defined in the S-57 format description. | | | | | | | | | | |
| **Message** | Subfield value does not conform to S-57 format specification. | | | | | | | | | | |
| **Solution** | Amend subfield value. | | | | | **Conformity** | | Part 3 (7.2.2.1) and (7.3) | | | |
| **Test Case No. 1** | Revised RUIN subfield in VRID | | | | | | | | | | |
| **Location** | | **Feature** | **Attributes** | | **FRID** | | **FOID** | | | **VRID** | |
|  | |  |  | |  | |  | | |  | |
| **Location** | - | | | **S57 Encoding** | | - | |  | | | |
| **FOID or VRID** | VE-0000000016 | | |  | |  | |  | | | |
| **Screen Capture** |  | | | | | | | | | | |
| **Expected Test Results** | 26a: An error “Subfield value does not conform to S-57 format specification” should be triggered. | | | | | | | | | | |
| **Secondary Critical Errors** | None | | | | | | | | | | |
|  | | | | | | | | | | | |
| **Dataset Name** | AA400015 | | | **S‐58 Check** | | 536 | | | **Type** | | C |
| **S-58 Description** | If a field without a repetition factor repeats. | | | | | | | | | | |
| **Message** | Field without a repetition factor repeats. | | | | | | | | | | |
| **Solution** | Remove repeating value. | | | | | **Conformity** | | 6.1.3 | | | |
| **Test Case No. 1** | Repeated the DSPM field records. | | | | | | | | | | |
| **Location** | | **Feature** | **Attributes** | | **FRID** | | **FOID** | | | **VRID** | |
|  | |  |  | |  | |  | | |  | |
| **Location** | - | | | **S57 Encoding** | | - | |  | | | |
| **FOID or VRID** | - | | |  | |  | |  | | | |
| **Screen Capture** |  | | | | | | | | | | |
| **Expected Test Results** | 536: An error “Field without a repetition factor repeats” should be triggered. | | | | | | | | | | |
| **Secondary Critical Errors** | None | | | | | | | | | | |
|  | | | | | | | | | | | |
| **Dataset Name** | AA400015 | | | **S‐58 Check** | | 540a | | | **Type** | | C |
| **S-58 Description** | If mandatory records, fields and subfields are not Present OR are Null where the “Null” value is not allowed. | | | | | | | | | | |
| **Message** | Mandatory records, fields or subfields are not used. | | | | | | | | | | |
| **Solution** | Add mandatory records/values. | | | | | **Conformity** | | 6.1.4, 6.3 and 6.4 | | | |
| **Test Case No. 1** | Removed XCOO subfield | | | | | | | | | | |
| **Location** | | **Feature** | **Attributes** | | **FRID** | | **FOID** | | | **VRID** | |
|  | |  |  | |  | |  | | |  | |
| **Location** | - | | | **S57 Encoding** | | - | |  | | | |
| **FOID or VRID** | - | | |  | |  | |  | | | |
| **Screen Capture** |  | | | | | | | | | | |
| **Expected Test Results** | 540a: An error “Mandatory records, fields or subfields are not used” must be triggered. | | | | | | | | | | |
| **Secondary Critical Errors** | None | | | | | | | | | | |
|  | | | | | | | | | | | |
| **Dataset Name** | AA400015 | | | **S‐58 Check** | | 540b | | | **Type** | | C |
| **S-58 Description** | If data set file contains prohibited records, fields or subfields. | | | | | | | | | | |
| **Message** | Prohibited records, fields or subfields used. | | | | | | | | | | |
| **Solution** | Remove prohibited records/values. | | | | | **Conformity** | | 6.3 and 6.4 | | | |
| **Test Case No. 1** | Added text for prohibited subfield “PSDN”. | | | | | | | | | | |
| **Location** | | **Feature** | **Attributes** | | **FRID** | | **FOID** | | | **VRID** | |
|  | |  |  | |  | |  | | |  | |
| **Location** | - | | | **S57 Encoding** | | - | |  | | | |
| **FOID or VRID** | - | | |  | |  | |  | | | |
| **Screen Capture** |  | | | | | | | | | | |
| **Expected Test Results** | 540b: An error “Prohibited records, fields or subfields used” must be triggered. | | | | | | | | | | |
| **Secondary Critical Errors** | None | | | | | | | | | | |