1. **Test Dataset: AA500017**

**S‐58 Recommended ENC Validation Checks covered in this section:**

|  |  |
| --- | --- |
| **S‐58 Check** | **Description** |
| 1014 | If the directory structure for physical media is not in accordance with the ENC Product Specification. |

**Secondary Errors** - None

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Dataset Name** | AA500017 | **S‐58 Check** | 1014 | | **Type** | C |
| **S-58 Description** | If the directory structure for physical media is not in accordance with the ENC Product specification. | | | | | |
| **Message** | The directory structure for physical media is not in accordance with the ENC Product Specification. | | | | | |
| **Solution** | Correct the directory structure of the physical media. | | **Conformity** | Appendix B.1  (5.4.3) | | |
| **Test Case No. 1** | Relocated README.TXT file outside of the ENC\_ROOT directory. | | | | | |
| **Expected Test Results** | 1014: An error “The directory structure for physical media is not in accordance with the ENC Product Specification” should be triggered. | | | | | |
| **Secondary Critical Errors** | None | | | | | |
| **Test Case No. 2** | Relocated the update (ER) file (AA5000017.001) outside of the ENC\_ROOT directory. | | | | | |
| **Expected Test Results** | 1014: An error “The directory structure for physical media is not in accordance with the ENC Product Specification” should be triggered. | | | | | |
| **Secondary Critical Errors** | None | | | | | |
| **Test Case No. 3** | Relocated the base (EN) file (AA5000017.000) outside of the ENC\_ROOT directory. | | | | | |
| **Expected Test Results** | 1014: An error “The directory structure for physical media is not in accordance with the ENC Product Specification” should be triggered. | | | | | |
| **Secondary Critical Errors** | None | | | | | |
| **Test Case No. 4** | Relocated the catalogue file (CATALOG.031) outside of the ENC\_ROOT directory. | | | | | |
| **Expected Test Results** | 1014: An error “The directory structure for physical media is not in accordance with the ENC Product Specification” should be triggered. | | | | | |
| **Secondary Critical Errors** | None | | | | | |
| **Test Case No. 5** | Renamed the ENC\_ROOT directory ‘ENC\_FILE. | | | | | |
| **Expected Test Results** | 1014: An error “The directory structure for physical media is not in accordance with the ENC Product Specification” should be triggered. | | | | | |
| **Secondary Critical Errors** | None | | | | | |